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1PV6

Here you can enable and configure the IPV6 support of the FRITZ!Box.

1PV6 Support
) 1Pv6 support enabled
1PV6 Connectivity
© Always use a native IPv4 connection (recommended)

First anative IPv4 connection is established. If a 6RD server address was learned through DHCP, a 6RD tunnel is established.
the device will attempt to establish a native IPv6 connection (Dual Stack).

© Always use a native IPv6 connection

For this operation mode your Internet service provider must support native IPv6 on your line.

© Always use a tunnel protocol for the IPv6 connection

Use IPv6 with a tunnel protocol over a conventional IPv4 connection. To use this operating mode your Internet service provic
have to support IPv6.

Additional Settings
O Set MTU manually[1280 Bytes





